From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Micha=C5=82=20Dzieko=C5=84ski?=
 <michal.dziekonski+github@gmail.com>
Date: Wed, 3 May 2023 12:17:28 +0000
Subject: arm64: dts: allwinner: h616: Fix thermal zones (add missing trips)

Signed-off-by: Michal Dziekonski <michal.dziekonski+github@gmail.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi | 29 ++++++++++
 1 file changed, 29 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
index 8628a9e3dfca..17b13d3193cc 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
@@ -877,6 +877,11 @@ cpu_target: trip-point@1 {
 					type = "passive";
 					hysteresis = <0>;
 				};
+				cpu_temp_critical: trip-point@2 {
+					temperature = <110000>;
+					type = "critical";
+					hysteresis = <0>;
+				};
 			};
 
 			cooling-maps {
@@ -895,18 +900,42 @@ gpu-thermal {
 			polling-delay = <1000>;
 			thermal-sensors = <&ths 0>;
 			sustainable-power = <1100>;
+
+			trips {
+				gpu_temp_critical: trip-point@0 {
+					temperature = <110000>;
+					type = "critical";
+					hysteresis = <0>;
+				};
+			};
 		};
 
 		ve-thermal {
 			polling-delay-passive = <0>;
 			polling-delay = <0>;
 			thermal-sensors = <&ths 1>;
+
+			trips {
+				ve_temp_critical: trip-point@0 {
+					temperature = <110000>;
+					type = "critical";
+					hysteresis = <0>;
+				};
+			};
 		};
 
 		ddr-thermal {
 			polling-delay-passive = <0>;
 			polling-delay = <0>;
 			thermal-sensors = <&ths 3>;
+
+			trips {
+				ddr_temp_critical: trip-point@0 {
+					temperature = <110000>;
+					type = "critical";
+					hysteresis = <0>;
+				};
+			};
 		};
 	};
 };
-- 
Armbian

