From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Kali Prasad <kprasadvnsi@protonmail.com>
Date: Sun, 19 Sep 2021 08:02:27 +0000
Subject: arm64: dts: allwinner: h616: Add device node for SID

The device tree binding for H616's SID controller.

Signed-off-by: Kali Prasad <kprasadvnsi@protonmail.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi | 15 ++++++++++
 1 file changed, 15 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
index 45359b0d317a..7ad1982fb47f 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
@@ -171,6 +171,21 @@ ccu: clock@3001000 {
 			#reset-cells = <1>;
 		};
 
+		sid: efuse@3006000 {
+			compatible = "allwinner,sun50i-h616-sid";
+			reg = <0x03006000 0x1000>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			cpu_speed_grade: cpu-speed-grade@0 {
+				reg = <0x00 0x02>;
+			};
+
+			ths_calibration: thermal-sensor-calibration@14 {
+				reg = <0x14 0x8>;
+			};
+		};
+
 		watchdog: watchdog@30090a0 {
 			compatible = "allwinner,sun50i-h616-wdt",
 				     "allwinner,sun6i-a31-wdt";
-- 
Armbian

