From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Sat, 16 Apr 2022 11:51:35 +0300
Subject: add nodes for sunxi-info, sunxi-addr and sunxi-dump-reg

---
 arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi | 19 ++++++++++
 1 file changed, 19 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
index 538c90663602..6365cce07304 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
@@ -1243,6 +1243,25 @@ ths: thermal-sensor@5070400 {
 			nvmem-cell-names = "calibration";
 			#thermal-sensor-cells = <1>;
 		};
+
+		sunxi-info {
+			compatible = "allwinner,sun50i-h6-sys-info";
+			status = "okay";
+		};
+
+		addr_mgt: addr-mgt {
+			compatible = "allwinner,sunxi-addr_mgt";
+			type_addr_wifi = <0x2>;
+			type_addr_bt = <0x2>;
+			type_addr_eth = <0x2>;
+			status = "okay";
+		};
+
+		dump_reg: dump_reg@20000 {
+			compatible = "allwinner,sunxi-dump-reg";
+			reg = <0x0 0x03001000 0x0 0x0f20>;
+			status = "okay";
+		};
 	};
 
 	thermal-zones {
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
index 98735d39e6e8..5ff1b357a25b 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
@@ -1053,6 +1053,25 @@ ths: thermal-sensor@5070400 {
 			nvmem-cell-names = "calibration";
 			#thermal-sensor-cells = <1>;
 		};
+
+		dump_reg: dump_reg@20000 {
+			compatible = "allwinner,sunxi-dump-reg";
+			reg = <0x0 0x03001000 0x0 0x0f20>;
+			status = "okay";
+		};
+
+		sunxi-info {
+			compatible = "allwinner,sun50i-h616-sys-info";
+			status = "okay";
+		};
+
+		addr_mgt: addr-mgt {
+			compatible = "allwinner,sunxi-addr_mgt";
+			type_addr_wifi = <0x2>;
+			type_addr_bt = <0x2>;
+			type_addr_eth = <0x2>;
+			status = "okay";
+		};
 	};
 
 	thermal-zones {
-- 
Armbian

